{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":35,"n_cols":11,"rows_kept":35,"merged":[[0,0,0,10],[31,0,31,10],[32,0,32,10]],"flags":["formulas_cached_only"]}
[" 泰州综合管廊材料申购表（2019年度）"]
["锦宸集团有限公司泰州综合管廊工程项目部"]
["序号 ","材料名称","型号及规格","材料","单位","数量","材料采购价（含税价）","材料品牌要求","钢管防腐要求"," 用途","备注"]
[1,"钢管（满足饮用水卫生要求）","D630*9","Q235","米",53,null,"天津友发、徐州光环、无锡湖光","钢管防腐要求见备注 钢管外防腐一底一布四油","管廊外给水","钢管长度需扣除管件、阀门所占的长度"]
[2,"钢管（满足饮用水卫生要求）","D530*9","Q235","米",110,null,"天津友发、徐州光环、无锡湖光","钢管防腐要求见备注 钢管外防腐一底一布四油","管廊外给水","钢管长度需扣除管件、阀门所占的长度"]
[3,"钢管（满足饮用水卫生要求）","D325*8","Q235","米",1161,null,"天津友发、徐州光环、无锡湖光","钢管防腐要求见备注 钢管外防腐一底一布四油","管廊外给水","钢管长度需扣除管件、阀门所占的长度"]
[4,"钢管（满足饮用水卫生要求）","D159*6","Q235","米",324,null,"天津友发、徐州光环、无锡湖光","钢管防腐要求见备注 钢管外防腐一底一布四油","管廊外给水","钢管长度需扣除管件、阀门所占的长度"]
[5,"平插（1头法兰1头承插口）","DN500","铸铁","个",2,{"$nulls":3},"管廊外给水","配胶圈"]
[6,"D530*9弯头9°","D530*9","Q235","个",2,{"$nulls":3},"管廊外给水"]
[7,"D530*9弯头10°","D530*9","Q235","个",1,{"$nulls":3},"管廊外给水"]
[8,"D530*9弯头11°","D530*9","Q235","个",1,{"$nulls":3},"管廊外给水"]
[9,"D325*8弯头145°","D325*8","Q235","个",1,{"$nulls":3},"管廊外给水"]
[10,"D325*8弯头147°","D325*8","Q235","个",1,{"$nulls":3},"管廊外给水"]
[11,"D325*8弯头155°","D325*8","Q235","个",1,{"$nulls":3},"管廊外给水"]
[12,"D325*8弯头146°","D325*8","Q235","个",1,{"$nulls":3},"管廊外给水"]
[13,"盲堵","DN600","Q235","个",2,{"$nulls":3},"管廊外给水"]
[14,"盲堵","DN300","Q235","个",39,{"$nulls":3},"管廊外给水"]
[15,"盲堵","DN150 ","Q235","个",10,{"$nulls":3},"管廊外给水"]
[16,"法兰盘","DN600","Q235","片",2,{"$nulls":3},"管廊外给水"]
[17,"法兰盘","DN500","Q235","片",2,{"$nulls":3},"管廊外给水"]
[18,"法兰盘","DN300","Q235","片",39,{"$nulls":3},"管廊外给水"]
[19,"法兰盘","DN150 ","Q235","片",10,{"$nulls":3},"管廊外给水"]
[20,"法兰垫片","DN600","钢垫片或橡胶","片",45,{"$nulls":3},"管廊外给水"]
[21,"法兰垫片","DN500","钢垫片或橡胶","片",6,{"$nulls":3},"管廊外给水"]
[22,"法兰垫片","DN300","钢垫片或橡胶","片",117,{"$nulls":3},"管廊外给水"]
[23,"法兰垫片","DN150 ","钢垫片或橡胶","片",32,{"$nulls":3},"管廊外给水"]
[24,"法兰垫片","DN200","钢垫片或橡胶","片",18,{"$nulls":3},"管廊外给水"]
[25,"法兰垫片","DN80","钢垫片或橡胶","片",27,{"$nulls":3},"管廊外给水"]
[]
[]
[]
["备注：1、钢管内防腐：采用液体无毒环氧涂料，产品需具备国家卫生部颁发的饮用水卫生安全的许可证（有效期内），并符合《生活饮用水输配水设备及防护材料的安全评价标准》（GB/T17219-1998),钢管除锈及内防腐，施工和验收严格执（SYT0457-2010)《钢管管道液体环氧涂料内防腐层技术标准》及(GB50268-2008)《给水排水管道工程施工及验收规范》，其中干膜厚度不小于200um,两道底漆，两道面漆。                                                                                             2、管廊外埋地钢管外防腐：采用环氧煤沥青一底一布四油，厚度不低于0.4毫米，材料质量必须达到SYJ28-87《埋地钢质管道环氧煤沥青防腐层技术标准》的要求。                                                                                                                         "]
["审核：                  预算：                   现场：                  申报："]
[]
["                                                                            日期：   年    月    日"]